SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( M62-1357
	Comment ( Original Model&Texture by Vlasyuk Roma aka "RoM" )
	Type ( Engine )
	WagonShape ( M62-1357.s )
	Size ( 2.95m 4.8m 17.35m )
	Mass ( 126t )
	WheelRadius ( 0.525m )
	InertiaTensor ( Box ( 2.95m 4.8m 17.35m) )

	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 1.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 10cm )
		)
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 1.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 10cm )
		)
		Velocity ( 0.01m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
Inside (
                PassengerCabinFile ( M62-1357.s )
                PassengerCabinHeadPos ( -1.7 3.134 7.12 )
                RotationLimit ( 99 99 99 )
                Sound ( "m62-265eng.sms" )
		    StartDirection ( 0 -90 0 )
      )
	Adheasion ( 0.2 0.8 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*117t )
	DerailBufferForce ( 936kN )
	NumWheels ( 12 )
	Friction (
		100N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s	0		1
	)

	BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir" )
	BrakeSystemType( "Air_single_pipe" )\
	MaxHandbrakeForce( 13.5kN )
	MaxBrakeForce( 92kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 10 )
	MaxApplicationRate( 12 )
	MaxAuxilaryChargingRate( 4 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 57 )

	IntakePoint ( -0.5 0.5 FuelDiesel )

	Lights	(	12
		
		Light	(
			comment( Sphere of light medium )
			Type		( 1.0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.2 )
			FadeOut	( 0.2 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 50fbfae1 )
					Position ( 0 1.5 18 )
					Transition ( 0 )
					Radius ( 150 )
					Angle ( 10 )
					)
				)
			)
	Light	(
			comment( Sphere of light bright )
			Type		( 1.0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.3 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fffbfae1 )
					Position ( 0 3.5 28 )
					Transition ( 0 )
					Radius ( 360 )
					Angle ( 15 )
					)
				)
			)

		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffc040 )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ffffbb )
					Position ( -1.07 1.56 8.15 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.0 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Head Light Top Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ffffbb )
					Position ( 0.0 4.17 8.1 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.0 )
					)

				)
			)
		
		
		
		
		Light	(
			comment( Head Light Top Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( 0.0 4.17 8.1 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 1.0 )

					)
				)
			)

		Light	(
			comment( Head light left Bright )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 1.07 1.56 8.15 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Head light right Bright )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( -1.07 1.56 8.15 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Rear Head light left Red )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Coupling ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 90ff0000 )
					Position ( 1.40 1.50 -8.10 )
					Azimuth ( -180 -180 -180 )

					Transition ( 0 )
					Radius ( 0.40 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Rear Head light left Red )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Coupling ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 90ff0000 )
					Position ( 1.40 1.50 -8.10 )
					Azimuth ( -180 -180 -180 )

					Transition ( 0 )
					Radius ( 0.40 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Rear Head light left Red )
			Type( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 3 )
				Coupling ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 90ff0000 )
					Position ( 1.40 1.50 -8.10 )
					Azimuth ( -180 -180 -180 )

					Transition ( 0 )
					Radius ( 0.40 )
					Elevation ( 0.0 0.0 0.0 )

					)
				)
			)
		Light	(
			comment( Rear Head light right Red )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Coupling ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffc040 )
					Position ( -1.10 1.55 -8.14 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.60 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)


		)	
	
	Sound ( "m62-265eng.sms" )
	)

Engine ( M62-1357
	Effects
	(
		DieselSpecialEffects
		(
			Exhaust1
			(
                                 0.0 4.57 2.755
				0 1 0
				0.15
			)
                                   Exhaust2
			(
                                0.2 4.57 2.755
				0 1 0
				0.12
			) 
                                   Exhaust3
			(
                               -0.2 4.57 2.755
				0 1 0
				0.12
			)
		)
	)

      
      Wagon ( M62-1357 )
	Type ( Diesel )
	MaxPower ( 1471kW )
	MaxForce ( 396kN )
	MaxContinuousForce ( 216kN )
	MaxVelocity ( 64mph )
	MaxCurrent ( 1800A )
	WheelRadius ( 0.525m )
	Sanding ( 8mph )
	NumWheels ( 6 )
	Vigilance ( 1 )
	MaxTemperature ( 100 )
	MaxOilPressure ( 90 )

	AirBrakesAirCompressorPowerRating( 1.5 )
	AirBrakesMainMinResAirPressure( 56 )
	AirBrakesMainMaxAirPressure( 126 )
	AirBrakesMainResVolume( 8 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 106 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2.75 )
	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerMinPressureReduction( 0 )
	TrainBrakesControllerMinPressureReduction( 0 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 2.5 )
	EngineBrakesControllerMaxApplicationRate( 2 )
	TrainBrakesControllerMaxApplicationRate( 1 )
	EngineBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxReleaseRate( 1 )
	EngineBrakesControllerEmergencyApplicationRate( 15 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 76 )
	TrainBrakesControllerMaxSystemPressure( 76 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 25 )
	TrainBrakesControllerFullServicePressureDrop( 25 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent( 1 )
	
	CabView ( "tsrLoco_m62.cvf" )
	HeadOut ( 1.7 3.134 7.12 )

	MaxDieselLevel ( 3150l )
	DieselUsedPerHourAtMaxPower ( 175l )
	DieselUsedPerHourAtIdle ( 40l )

	DieselSmokeEffectInitialMagnitude( 0.7 )
	DieselSmokeEffectMaxMagnitude( 2.0 )
	DieselSmokeEffectInitialSmokeRate( 0.5 )
	DieselSmokeEffectMaxSmokeRate( 4.0 )

	DieselEngineIdleRPM( 660 )
	DieselEngineMaxRPM( 1500 )
	DieselEngineMaxRPMChangeRate( 90 )
	DieselEngineSpeedOfMaxTractiveEffort( 24mph )



	DoesHornTriggerBell( 0 )
	
	
	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 0 )
    		MonitoringDeviceAppliesShutsDownEngine( 1 )
    		)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 35 )
		MonitoringDeviceAlarmTimeLimit( 30 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)
		
	AWSMonitor(
		MonitoringDeviceMonitorTimeLimit( -1 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 92 )
		MonitoringDeviceResetLevel( 1 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed( 2 )
		MonitoringDeviceDoesSuppressionReset( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 4 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
        EngineControllers (
            Throttle ( 0 1 0.07 0
                NumNotches ( 16
                    Notch ( 0       0 Dummy )
                    Notch ( 0.07   0 Dummy )
                    Notch ( 0.14   0 Dummy )
                    Notch ( 0.21   0 Dummy )
                    Notch ( 0.28   0 Dummy )
                    Notch ( 0.35   0 Dummy )
                    Notch ( 0.42   0 Dummy )
                    Notch ( 0.49   0 Dummy )
                    Notch ( 0.56   0 Dummy )
                    Notch ( 0.63   0 Dummy )
                    Notch ( 0.70   0 Dummy )
                    Notch ( 0.77   0 Dummy )
                    Notch ( 0.84   0 Dummy )
                    Notch ( 0.90   0 Dummy )
                    Notch ( 0.95   0 Dummy )
                    Notch ( 1       0 Dummy )
                )
            )

		Brake_Engine ( 0 0.75 0.147 0.75
			NumNotches ( 5
			Notch ( 0        0 EngineBrakesControllerReleaseStart ) 
			Notch ( 0.147  0 EngineBrakesControllerApplyStart ) 
			Notch ( 0.293  0 EngineBrakesControllerApplyStart ) 
			Notch ( 0.517  0 EngineBrakesControllerApplyStart ) 
			Notch ( 0.750  0 EngineBrakesControllerApplyStart ) 
			)
		)
		Brake_Train ( 0 1 0.01 0.2 
			NumNotches ( 5
			Notch ( 0    0 TrainBrakesControllerReleaseStart )
			Notch ( 0.2  0 TrainBrakesControllerRunningStart )
			Notch ( 0.3  0 TrainBrakesControllerHoldLappedStart )
			Notch ( 0.9  0 TrainBrakesControllerFullServiceStart )
			Notch ( 1    0 TrainBrakesControllerEmergencyStart )
			)
		)

		DirControl ( -1 0 1 1 )
		EmergencyStopToggle( 0 1 0 )
		AWS ( 0 1 0 )
		Sanding ( 0 1 0 )
		Horn ( 0 1 0 )
		BellToggle( 0 1 0 )
		Vigilance ( 0 1 0 )
		Headlights ( 0 0.25 1 0 )
		Wipers ( 0 1 0 )
		BailOffButton( 0 1 0 )
        )

      Sound (	"m62-265cab.sms" )
    	Name ("M62-1357")
            Description (
	"Russian diesel-electric freight locomotive M62.\n\n"+
	"It is the most popular diesel locomotive"+
	"on Russian railroads. "+
	"Engine: 14-D40\n"+
	"Power: 1471 kWt\n"+
	"Max. speed: 100 km/h\n"+
	"Height: 4.95 m\n"+
	"Width:  2.95 m\n"+
	"Length: 17.4 m\n"+
	"Weight: 117 tons\n"+
	"Wheel configuration: 3Co"
    	)
    	EngineOperatingProcedures (
    	"To move forward\n"+
	"1.	Press the W key to move the Reverser to Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"4.	Press the D key to move the throttle from Idle to Notch 1.\n"+
	"5.	Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the dynamic brakes\n"+
	"1.	Press the A key to move the throttle to the Idle position.\n"+
	"2.	Wait for 10 seconds, then press the . (PERIOD) key to advance the Dynamic Brake handle from Off to the Setup position. After allowing a few seconds for braking circuit setup, press the . (PERIOD) key again to set the desired level of dynamic braking (Levels 1 - 8).\n\n"+
	"To release the dynamic brakes\n"+
	"1. Press the D key to move the throttle towards Idle.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
    	) 
)
